# JMR Automation Tire Wash Tub - Owner's Manual

## PRODUCT OVERVIEW

The JMR Automation Cordless Tire Wash Tub is a mobile, efficient solution for cleaning dirt modified tires. Powered by a Milwaukee M18 or DeWalt 20V battery, it's ideal for both at-the-track and shop use.

## FEATURES

* Cordless operation with Milwaukee M18 or DeWalt 20V battery (not included)
* Simple On/Off switch that illuminates when active
* 6.5-gallon water reservoir with overflow control
* Built-in stainless-steel brush continuously cleans rotating tire
* Nozzle manifold for optional garden hose spray
* Drain valve for easy emptying and flushing
* Heavy-duty casters for full mobility

## QUICK START INSTRUCTIONS

* Fill tub up to the drain hole with clean water.
* Install battery into click on switch box.
* Tilt the motor assembly back.
* Install tire on hub and loosely spin on lug nuts.
* Tilt the motor and tire assembly into tub.
* Turn the switch “ON” to start rotation and cleaning.

NOTE: You may connect a garden hose to the nozzle

manifold for more efficient cleaning.

You may also use the supplied brush to help

Clean the side walls, rim and tread of tire.

* Turn the switch to “OFF” when tire is sufficiently cleaned.
* Remove the tire from the system in the opposite order.
* After cleaning tires, open the front valve to drain water.
* Flush tub with clean water if needed and close valve.

## CLEANING & MAINTENANCE

* Drain after every use.
* Use only soap and low-pressure water for cleaning.
* Use garden hose for thorough flushing.
* Store in a dry environment.
* Inspect brushes and drain regularly for debris.

## SAFETY NOTES

* Use only Milwaukee M18 or DeWalt 20V batteries.
* Do not operate with loose or damaged parts.
* Keep away from children and pets.
* Do not put hands between the tire and tub sides.
* Do not use with pressure washing systems.